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3-way bass reflex
column speaker
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1 x 6-1/2" woofer
coated cellulose cone,
1" coil, 3-3/8" magnet 

1 x 6-1/2" mid-woofer
coated cellulose cone,
1" coil, 3-3/8" magnet

1 x Titanium inverted 
dome tweeter,
ferrofluid cooled 3/4" coil,
2-3/8" magnet
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52Hz - 22kHz
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91.5dB
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8 ohms
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3.4 ohms
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120Hz / 3.5kHz
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125W
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25-100W (into 8 ohms)
only mono wiring
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925x200x262mm
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15kg
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• Black ash
• Palisander
• Light oak 
[image: image19.png] Frontcover |




Black cloth
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1 x front circular port
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Floor standing
(4 spikes and cups included)



